5:70-3.2 Modifications

(a) The following articles or sections of the State Fire Prevention Code are modified as follows:

1. – 37. (No change.)

38. Chapter 38, Liquefied Petroleum Gases, shall be amended as follows:

i.- ix. (No change.)

x. New Section 3806.4, Labeling, shall be inserted as follows: "3806.4 Labeling. Prior to filling any cylinder 4 to 40 pounds LP-Gas capacity, except fork lift cylinders, the operator of the fill plant or distribution plant shall affix a label to the collar of the cylinder that includes the following warning printed in English and in Spanish: 'Flammable Gas - Never Use or Store Indoors/Gas Inflammable-Nunca Se Use o Guarde Adentro.' " **In ~~lieu of~~ addition to this verbal warning, a label approved by the Department that graphically depicts the prohibition on bringing a cylinder indoors ~~may~~ shall be affixed to the collar of the cylinder.**

xi. – xvii. (No change.)

 39. – 46. (No change.)